SPEEXENC(1)

NAME
speexenc - manual page for speexenc version 1.1

SYNOPSIS
speexenc [options] input_file output_file

DESCRIPTION
Encodes input_file using Speex. It can read the WAV or raw files.

  input_file can be:

filename.wav
    wav file

filename.*
    Raw PCM file (any extension other than .wav)

-   stdin

  output_file can be:

filename.spx
    Speex file

-   stdout

OPTIONS

-n, --narrowband
    Narrowband (8 kHz) input file

-w, --wideband
    Wideband (16 kHz) input file

-u, --ultra-wideband "Ultra-wideband" (32 kHz) input file

--quality n
    Encoding quality (0-10), default 8

--bitrate n
    Encoding bit-rate (use bit-rate n or lower)

--vbr
    Enable variable bit-rate (VBR)

--abr rate
    Enable average bit-rate (ABR) at rate bps

--vad
    Enable voice activity detection (VAD)

--dtx
    Enable file-based discontinuous transmission (DTX)

--comp n
    Set encoding complexity (0-10), default 3

--nframes n
    Number of frames per Ogg packet (1-10), default 1

--comment
    Add the given string as an extra comment. This may be used multiple times

--author
    Author of this track

--title
    Title for this track

-h, --help
    This help

-v, --version
    Version information

-V  Verbose mode (show bit-rate)

  Raw input options:

--rate n
    Sampling rate for raw input

--stereo
    Consider raw input as stereo

--le
    Raw input is little-endian

--be
    Raw input is big-endian

--8bit
    Raw input is 8-bit unsigned

--16bit
    Raw input is 16-bit signed

Default raw PCM input is 16-bit, little-endian, mono

More information is available from the Speex site: http://www.speex.org

Please report bugs to the mailing list `speex-dev@xiph.org'.

COPYRIGHT
Copyright © 2002 Jean-Marc Valin