************         BUILDCD and BCDFlat Readme file            *************
************                                                    *************
*****************************************************************************

Current Versions:

	BuildCD         2.26            September 04 1995
	BCDFlat         2.26            September 04 1995

+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
=============================================================================

BuildCD
-------

	16-bit version which allows full 32 channel interleaving as defined
	the ISO 9660 standard.

	Recent bug fixes / changes
	--------------------------

	2.27 Wrong size in directory record corrected. More updates to 
	     Cdgen o/p.

	2.26 Scrambling Error Resloved ?        

	2.25 Updated CDGen ouput.        

	2.23 -ve file size problem in map file for files over 33Mb removed. 
	
	1.22 Binary map record now output for gap.

	     SCSI errors described / displayed.

	1.21 -L non-interactive mode.


BCDFlat
-------

	32-bit DOS-extended version ( requires DOS4GW ). Limited to 20 open 
	files at present. Limits interleaving to between 15-18 channels, 
	depending on option chosen.

	Recent bug fixes / changes
	--------------------------
	
	2.27  Wrong directory size problem corrected. Updates to correct
	      o/p of .ccs files?
	
	2.26  Scrambling Error unlikely as updated code already implemented
	
	2.25  Updated CDGen output

	2.24  -m output without needing to generate an image.

	      Path location bug fixed.

	      Dir / Sub-dir screen garbarge / program crash fixed.

	2.23  -ve file size problem in map file for files over 33Mb removed. 
	
	      Binary map record now output for gap.

	      SCSI errors described / displayed.

	      -L non-interactive mode.


	

=============================================================================
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

From now on the features available in BuildCD and BCDFlat will be updated 
together along with any bug fixes. To account for this the version numbers
will be the same, the program being identified by the separate names. Until 
full 32 channel interleaving is available in BCDFlat it will be necessary to
use BuildCD in these instances.

If you have any problems with either of these programs contact SNSytems

e-mail support@snsys.com


04 September 1995.

